( TL19E00J54200014401KDAT00 )

Battery Removal/Installation

Installation

1. Install the battery (A), then install the battery cover (B) and battery setting plate (C).

1. Tighten the two nuts (D) equally until the battery is stable.
   NOTE: Do not deform the battery setting plate by tightening the nuts too much.

1. Do the battery terminal reconnection procedure.
   NOTE: Make sure the positive terminal and the negative terminal are not reverse-connected.