( TL19E2AK72100090443FAAT00 )

DTC Troubleshooting: P0443 (92)

DTC P0443:
EVAP Canister Purge Valve Circuit Malfunction
NOTE: Before you troubleshoot, record all freeze data and any on-board snapshot, and review the general troubleshooting information.

1. Turn the ignition switch to ON (II).

1. Clear the DTC with the HDS.

1. Start the engine. Hold the engine speed at 3,000 rpm (min −1 ) without load (A/T in P or N, M/T in neutral) until the radiator fan comes on, then let it idle.

1. Check for Temporary DTCs or DTCs with the HDS.

Is DTC P0443 indicated?

YES | - | Go to Step 5 .
NO | - | Intermittent failure, the system is OK at this time. Check for poor connections or loose terminals at the EVAP canister purge valve and the ECM/PCM.■

1. Turn the ignition switch to LOCK (0), and allow the engine to cool below 60 °C (140 °F).

1. Disconnect the vacuum hose (A) from the EVAP canister purge valve (B) in the engine compartment, and connect a vacuum pump/gauge to the hose.

1. Start the engine, and let it idle.

Is there vacuum?

YES | - | Go to Step 8 .
NO | - | Go to Step 14 .

1. Turn the ignition switch to LOCK (0).

1. Disconnect the EVAP canister purge valve 2P connector.

1. Check for continuity between EVAP canister purge valve 2P connector terminal No. 2 and body ground.

Is there continuity?

YES | - | Go to Step 11 .
NO | - | Go to Step 23 .

1. Jump the SCS line with the HDS.

1. Disconnect ECM/PCM connector B (44P).

1. Check for continuity between EVAP canister purge valve 2P connector terminal No. 2 and body ground.

Is there continuity?

YES | - | Repair short in the wire between the EVAP canister purge valve and the ECM/PCM (B3), then go to Step 24 .
NO | - | Go to Step 30 .

1. Turn the ignition switch to LOCK (0).

1. Disconnect the EVAP canister purge valve 2P connector.

1. Turn the ignition switch to ON (II).

1. Measure the voltage between EVAP canister purge valve 2P connector terminal No. 1 and body ground.

Is there battery voltage?

YES | - | Go to Step 18 .
NO | - | Repair open in the wire between the EVAP canister purge valve and the No. 7 ACG (15A) fuse in the driver's under-dash fuse/relay box, then go to Step 24 .

1. Turn the ignition switch to LOCK (0).

1. Jump the SCS line with the HDS.

1. Disconnect ECM/PCM connector B (44P).

1. Check for continuity between ECM/PCM connector terminal B3 and EVAP canister purge valve 2P connector terminal No. 2.

Is there continuity?

YES | - | Go to Step 22 .
NO | - | Repair open in the wire between the EVAP canister purge valve and the ECM/PCM (B3), then go to Step 24 .

1. Measure the resistance between EVAP canister purge valve 2P connector terminals No. 1 and No. 2.

Is there about 23−26 Ω at room temperature?

YES | - | Go to Step 30 .
NO | - | Go to Step 23 .

1. Replace the EVAP canister purge valve.

1. Reconnect all connectors.

1. Turn the ignition switch to ON (II).

1. Reset the ECM/PCM with the HDS.

1. Do the ECM/PCM idle learn procedure.

1. Check for Temporary DTCs or DTCs with the HDS.

Is DTC P0443 indicated?

YES | - | Check for poor connections or loose terminals at the EVAP canister purge valve and the ECM/PCM, then go to Step 1 .
NO | - | Go to Step 29 .

1. Monitor the OBD STATUS for DTC P0443 in the DTCs MENU with the HDS.

Does the screen indicate PASSED?

YES | - | Troubleshooting is complete. If any other Temporary DTCs or DTCs were indicated in Step 28 , go to the indicated DTC's troubleshooting.■
NO | - | If the screen indicates FAILED, check for poor connections or loose terminals at the EVAP canister purge valve and the ECM/PCM, then go to Step 1 . If the screen indicates EXECUTING, keep idling until a result comes on. If the screen indicates OUT OF CONDITION or NOT COMPLETED, go to Step 27 .

1. Reconnect all connectors.

1. Update the ECM/PCM if it does not have the latest software, or substitute a known-good ECM/PCM.

1. Start the engine.

1. Check for Temporary DTCs or DTCs with the HDS.

Is DTC P0443 indicated?

YES | - | Check for poor connections or loose terminals at the EVAP canister purge valve and the ECM/PCM. If the ECM/PCM was updated, substitute a known-good ECM/PCM, then go to Step 32 . If the ECM/PCM was substituted, go to Step 1 .
NO | - | Go to Step 34 .

1. Monitor the OBD STATUS for DTC P0443 in the DTCs MENU with the HDS.

Does the screen indicate PASSED?

YES | - | If the ECM/PCM was updated, troubleshooting is complete. If the ECM/PCM was substituted, replace the original ECM/PCM. If any other Temporary DTCs or DTCs were indicated in Step 23 , go to the indicated DTC's troubleshooting.■
NO | - | If the screen indicates FAILED, check for poor connections or loose terminals at the EVAP canister purge valve and the ECM/PCM. If the ECM/PCM was updated, substitute a known-good ECM/PCM, then go to Step 32 . If the ECM/PCM was substituted, go to Step 1 . If the screen indicates EXECUTING, keep idling until a result comes on. If the screen indicates OUT OF CONDITION or NOT COMPLETED, go to Step 32 .