( TL19E00J26220257121KDAT00 )

Dashboard/Steering Hanger Beam Removal/Installation

Middle portion (shift lever portion)

1. Disconnect the floor wire harness connector (A) on some RHD models, the SRS unit connector (B), the parking brake switch connector (C), the yaw rate-lateral acceleration sensor connector (D), and if equipped, the USB adapter unit connector (E), and detach the wire harness clips (F). Using a TORX T30 bit, remove the ground bolt (G).

LHD model
RHD model