( TL19E00K76A000Y11A2FAAT00 )

DTC Troubleshooting: B11A2

DTC B11A2:
Passenger's MICU (EEPROM) Error

1. Clear the DTCs with the HDS.

1. Turn the ignition switch to LOCK (0) and then back to ON (II).

1. Wait for 6 seconds or more.

1. Check for DTCs with the HDS.

Is DTC B11A2 indicated?

YES | - | Faulty passenger's MICU, replace the passenger's under-dash fuse/relay box.■
NO | - | Intermittent failure, the system is OK at this time.■