( TL19E00J46643421011FEAT00 )

Door Lock Knob Switch Test

Driver's Door

1. Remove the driver's door panel.

1. Disconnect the 10P connector (A) from the actuator (B).

1. Check for continuity between the terminals.
   - There should be continuity between the No. 6 [No. 9] and No. 5 [No. 10] terminals when the door lock knob switch is in the LOCK position and no continuity when the switch is in the UNLOCK position.
   - There should be continuity between the No. 7 [No. 8] and No. 5 [No. 10] terminals when the door lock knob switch is in the UNLOCK position and no continuity when the switch is in the LOCK position.
   [ ]: RHD model

1. If the continuity is not as specified, replace the door lock actuator.