( TL19E00H46400012802BAAT00 )

Airbag and Tensioner Disposal

Deploying Airbags in the Vehicle
Special Tools Required
Deployment tool
07HAZ-SG00500
Before scrapping any airbags, side airbags, side curtain airbags, or seat belt tensioners (including those in a whole vehicle to be scrapped), the part(s) must be deployed. If the vehicle is still within the warranty period, the Honda District Parts and Service Manager must give approval and/or special instruction before deploying the part(s). Only after the part(s) have been deployed (as the result of vehicle collision, for example), can they be scrapped. If the parts appear intact (not deployed), treat them with extreme caution. Follow this procedure.
If an SRS equipped vehicle is to be entirely scrapped, its airbags, side airbags, side curtain airbags, and seat belt tensioners, should be deployed while still in the vehicle. These parts should not be considered as salvageable parts and should never be installed in another vehicle.

1. Turn the ignition switch to LOCK (0). Do the battery terminal disconnection procedure, then wait for 3 minutes before starting work.

1. Confirm that each airbag, side airbag, side curtain airbag, or seat belt tensioner is securely mounted.

1. Confirm that the deployment tool is functioning properly by following the check procedure on the tool label.

Driver's Airbag

1. Remove the access panel (A) from the steering wheel then disconnect the driver's airbag 4P connector (B) from the cable reel.