( TL19E00J26273450001KDAT00 )

Interior Trim Removal/Installation - Rear Shelf Area

Rear Speaker Grille
NOTE:

- Take care not to bend or scratch the rear shelf and the trim.
- When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.

1. Remove the rear speaker grille (A). The left side is shown; the right side is symmetrical.

   -1. | Using a flat-tip screwdriver wrapped with protective tape, pry up the notch (B) of the grille to detach the hook (C).
   -2. | Pull up along the edge of the grille to detach the clips and the hooks (D).
   -3. | Pull the grille back to release the hooks (E) from the rear shelf (F).

1. Install the grille in the reverse order of removal, and note these items:
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Push the clips and the hooks into place securely.