( TL19E00J46166400000KDAT00 )

Rear Seat Removal/Installation

Seat Cushion
NOTE: Take care not to scratch the body or tear the seat covers.

1. Fold both rear seat-backs forward.

1. For some models: Pull back the front portion of the spare tyre lid, and detach the clips:
   - With temporary repair kit (TRK)/with compact spare tyre
   - With normal spare tyre

1. Remove the bolt securing the seat cushion (A) from behind the left rear seat-back (B).

1. Raise both rear seat-backs.