( TL19E1PE10436445401FEAT00 )

A/T Interlock System - Park Pin Switch Test

1. Remove the center console.

1. Disconnect the shift lever 6P connector.

1. Shift into P, and check for continuity between park pin switch/A/T gear position indicator panel light connector terminals No. 1 and No. 2.
   There should be no continuity.

1. Shift out of P, and check for continuity between connector terminals No. 1 and No. 2.
   There should be continuity.

1. If the park pin switch tests OK.
   If the park pin switch fails the test, replace the park pin switch; LHD model, RHD model.

1. Install the center console.