( TL19E1AE34116300000KBAT00 )

Clutch Replacement

1. Torque the mounting bolts (A) in a crisscross pattern. Tighten the bolts in several steps to prevent warping the diaphragm spring.

   Specified Torque: | 25 N·m (2.6 kgf·m, 19 lbf·ft)

1. Remove the ring gear holder (B) and the shaft (clutch alignment tool) (C), the taper cone (clutch alignment tool) (D), and the 21 mm clutch alignment pilot.

1. Make sure the diaphragm spring fingers are all the same height.

1. Do the release bearing inspection, and replace if it necessary.

1. Install the transmission: R20A3 engine model, K24Z3 engine model.