( TL19E1PE10411239511KCAT00 )

A/T Housing Bearing Installation

1. Expand each snap ring using snap ring pliers, and install the idler gear shaft bearing (A) and the secondary shaft bearing (B) part-way into the transmission housing using the 15 x 135L driver handle and the 42 x 47 mm bearing driver attachment.

1. Release snap ring pliers, then push the bearing down into the transmission housing until the snap ring snaps in place around it.