( TL19E00J32133100000FAAT00 )

HID Lamp System Troubleshooting

1. Measure the voltage between the No. 2 terminal of the HID unit 2P connector and body ground.

Is there battery voltage?

YES | - | Go to Step 14 .

NO

-

Repair open in the wire between the HID unit and driver's under-dash fuse/relay box (or passenger's under-dash fuse/relay box). If the wire is OK, replace the appropriate under-dash fuse/relay box, then go to Step 15 .

- Driver's under-dash fuse/relay box
- Passenger's under-dash fuse/relay box