( TL19E00K773000Y1829FAAT00 )

DTC Troubleshooting: B1829

DTC B1829:
A/T P Signal and VSS Signal Mismatch

1. Clear the DTCs with the HDS.

1. Start the engine.

1. Test drive at 10 km/h (6 mph) for 10 seconds.

1. Check for the DTCs with the HDS.

Is DTC B1829 indicated?

YES | - | Go to Step 5 .
NO | - | Intermittent failure, the system is OK at this time. Check for loose or poor connections.■

1. Check the P indicator of the shift position indicator and the MIL.

Does the P indicator and MIL come on?

YES | - | Troubleshoot the automatic transmission system.■
NO | - | Go to Step 6 .

1. Check for the gauge control module DTCs with the HDS.

Are there any DTCs indicated?

YES | - | Go to the indicated DTC's troubleshooting.■
NO | - | Replace the power seat control unit .■