( TL19E00J54400050461KBAT00 )

Rear Window Replacement

1. Apply primer to the edge of the rear window (A) where the lower rubber dam adhesive tape will be attached as shown. Attach the lower rubber dam (B) with adhesive tape (C) to the lower edge of the rear window:
   - After installing the rubber dam, cut the ends (D) of the rubber dam as shown.
   - Be careful not to touch the windshield where adhesive will be applied.

   Lower rubber dam adhesive tape:
   | Thickness 0.2 mm (0.008 in.)
   | Width 4 mm (0.16 in.)