( TL19E00J36100000000FAAT08 )

Navigation System Symptom Troubleshooting - Picture has lines or rolls

Picture has lines or rolls
Diagnostic Test: Monitor Check
NOTE:

- Always compare the screen image to a known-good vehicle. If the screen looks the same, inform the customer that it is a characteristic of the system.
- Check the connectors for poor connections or loose terminals.
- Make sure that the correct version are installed.
- Inspect the DVD for dirt or damage.
- Check any official Honda service website for more service information about the navigation system.
- Check the navigation screen settings for brightness, contrast, and black level, and check the color screen for map color and menu color.
- Before troubleshooting, make sure you have anti-theft codes for the audio system and the navigation system.
- After troubleshooting, enter the anti-theft codes for the audio system and the navigation system.
- Check the vehicle battery condition first.

1. Check for electronic aftermarket accessories (possibly hidden) mounted near the navigation display unit or the navigation unit.

Are there any electronic accessories?

YES | - | Disable the accessories, and recheck.■
NO | - | Go to Step 2 .

1. Start up the navigation picture.

Is the picture scrolling horizontally (left to right or right to left)?

YES | - | Check for an open or short to ground in the C SIG wire from navigation unit connector B (32P) No. 18 terminal to navigation display unit 28P connector No. 23 terminal. Also check for a short to ground between navigation display unit 28P connector No. 23 and No. 24 terminals.■
NO | - | Go to Step 3 .

1. Go into the Detail Information & Settings select Monitor Check, and use RGB Color diagnostic under Monitor Check.

Is the picture missing a red, green or blue color?

YES | - | Do troubleshooting for the picture is missing a color or tone or is an odd color. ■
NO | - | Go to Step 4 .

1. Turn the ignition switch to LOCK (0).

1. Substitute a known-good navigation display unit, and recheck.

Is the picture OK?

YES | - | Check for loose connections, then replace the original navigation display unit. ■
NO | - | Check for loose connections and recheck. If a poor connection or loose terminal is found, replace the shielded harness. If no poor or loose terminals are found, substitute a known-good navigation unit and recheck. If the problem is gone, replace the original navigation unit. ■