( TL19E00H46200053401KBAT00 )

Front Seat Belt Replacement

Front Seat Belt
SRS components are located in this area. Review the SRS component locations and the precautions and procedures before doing repairs or service.
NOTE:

- Check the front seat belts for damage, and replace them if necessary.
- LHD model is shown; RHD model is symmetrical.

1. Driver's side: Prepare a sheet of cardboard which is 2−2.5 mm (0.08−0.1 in.) thick.
   NOTE: If there is no suitable cardboard, put some seats of thin paper together until they will be required thick.

1. Driver's side: Make a jig (A) from the prepared cardboard (B).

1. Do the battery terminal disconnection procedure, then wait at least 3 minutes before beginning work.

1. Slide the front seat forward fully.

Dimensions of the jig