( TL19E00K791000R421XFAAT00 )

DTC Troubleshooting: 42-1x

1. Measure the voltage between the No. 38 terminal of SRS unit connector A (39P) and body ground, and between the No. 39 terminal and body ground. There should be less than 1 V.

Is the voltage as specified?

YES | - | Go to Step 15 .
NO | - | Short to power in the right engine compartment wire harness or dashboard wire harness; replace the faulty harness.■

1. Turn the ignition switch to LOCK (0).