( TL19E00J54300065705KBAT00 )

Wiper Blade Replacement

Installation

1. Align the groove (A) of the each rail (B) and a new blade (C).

1. Install the new blade with the rails into the blade holder in the reverse order of removal.

1. Install the wiper blades assemblies onto the wiper arms in the reverse order of removal.

1. Test the wipers by turning the wiper switch on. If the blades slip, turn the wiper switch off and seat the wiper blade securely.