( TL19E1AE34100041701MDAT00 )

MTF Inspection and Replacement

1. If the MTF is dirty, remove the drain plug (A), sealing washer (B) and drain the MTF.

1. Install the drain plug with a new sealing washer, and refill the MTF to the proper level. Always use genuine Honda Manual Transmission Fluid (MTF).

   Fluid Capacity
   | 1.9 L (2.0 US qt, 1.7 lmp qt) at fluid change
   | 2.0 L (2.1 US qt, 1.8 lmp qt) at overhaul

1. Install the filler plug (C) with a new sealing washer (D).

R20A3 engine model
K24Z3 engine model