( TL19E30A14666351511FEAT00 )

VTEC Rocker Arm Test

Special Tools Required
Air supply, 3/8
07LAJ-PR30102
VTEC air adapter
07ZAJ-PNA0101
VTEC air stopper
070AJ-0030100
Air joint adapter
07ZAJ-PNA0300

1. Start the engine, and let it run for 5 minutes, then turn the ignition switch to LOCK (0).

1. Remove the cylinder head cover.

1. Set the No. 1 piston at top dead center (TDC).

1. Move the secondary rocker arm (A) for the No. 1 cylinder. The secondary rocker arm should move independently of the mid rocker arm (B).
   - If the secondary rocker arm does not move, remove the mid, primary, and secondary rocker arms as an assembly, and check that the pistons in the rocker arms move smoothly. If any rocker arm needs replacing, replace the mid, primary, and secondary rocker arms as an assembly, then retest.
   - If the secondary rocker arm moves freely, go to Step 5 .

1. Repeat Step 4 on the remaining secondary rocker arms with each piston at TDC. When all the secondary rocker arms pass the test, go to Step 6 .

1. Check that the air pressure on the shop air compressor gauge indicates over 400 kPa (4.0 kgf/cm 2 , 57 psi).

1. Inspect the valve clearance.

1. Remove the sealing bolt (A) from the relief hole, and install the VTEC air stopper (B).

1. Remove the No. 2 and No. 3 camshaft holder bolts, and install the VTEC air adapters (C) finger-tight.

1. Connect the air joint adapter (D) and the air supply (E).

1. Loosen the valve on the regulator, and apply the specified air pressure.

   Specified Air Pressure:
   290 kPa (3.0 kgf/cm 2 , 42 psi)

   NOTE: If the rocker arm piston does not move after applying air pressure; move the rocker arm up and down manually by rotating the crankshaft clockwise.

1. With the specified air pressure applied, move the secondary rocker arm (A) for the No. 1 cylinder. The mid rocker arm (B), primary rocker arm (C), and secondary rocker arm should move together.
   - If the mid and primary rocker arms do not move together with the secondary rocker arm, remove the mid, primary, and secondary rocker arms as an assembly, and check that the pistons in the rocker arms move smoothly. If any rocker arm needs replacing, replace the mid, primary, and secondary rocker arms as an assembly, then retest.

1. Repeat Step 12 on the remaining secondary rocker arms with each piston at TDC. When all the secondary rocker arms pass the test, go to Step 14 .

1. Remove the air supply, the air joint adapter, the VTEC air adapters, and the VTEC air stopper.

1. Tighten the camshaft holder mounting bolts to 22 N·m (2.2 kgf·m, 16 lbf·ft).

1. Tighten the sealing bolt to 10 N·m (1.0 kgf·m, 7.4 lbf·ft).

1. Install the cylinder head cover.