( TL19E00D14300014801MBAT00 )

Brake Pedal and Brake Pedal Position Switch Adjustment

Pedal Height

1. Remove the driver's dashboard undercover.

1. Turn the brake pedal position switch (A) counterclockwise, and pull it back until it is no longer touching the brake pedal.

1. Remove the footrest, then remove the steering joint cover.

1. Pull back the carpet and find the cutout (B) in the insulation. Measure the pedal height (C) at the center of the pedal pad (D) to the floor without the insulation.

   Standard pedal height (with carpet removed):
   | LHD model:
   | M/T: | 164 mm (6.46 in.)
   | A/T: | 173 mm (6.81 in.)
   | RHD model:
   | M/T: | 167 mm (6.57 in.)
   | A/T: | 172 mm (6.77 in.)