( TL19E1PE10410459801KCAT00 )

A/T Shaft Assembly and Housing Installation

1. Install the three dowel pins (A) and a new gasket (B) on the torque converter housing (C).

1. Align the spring pin of the selector control shaft (D) with the transmission housing groove (E) by turning the selector control shaft on the torque converter side.
   NOTE: Do not squeeze the end of the selector control shaft tips together when turning the selector control shaft. If the selector control shaft tips are squeezed together, it will cause a faulty shift position signal or position due to the play between the selector control shaft and the transmission range switch.

1. Place the transmission housing (F) on the torque converter housing. Do not install the input shaft (mainshaft) speed sensor and the output shaft (countershaft) speed sensor before installing the transmission housing on the torque converter housing.