( TL19E00J26220230101KDAT00 )

Glove Box Removal/Installation

1. Pull the glove box (A) by hand to detach the clips, disconnect the glove box light connector (B) and the trunk lid opener main switch connector (C), then remove the glove box.

1. Install the glove box in the reverse order of removal, and note these items:
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Make sure each connector is plugged in properly.
   - Push the clips and the hooks into place securely.