( TL19E00J26273421601KDAT00 )

Interior Trim Removal/Installation - Door Areas

1. Pull out the front door opening seal (A) from the trim hooks (B) and around the front door opening flange, then remove the seal.

1. Install the trim in the reverse order of removal, and note these items:
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Push the clips, the hooks, and the tabs into place securely.