( TL19E00J26200031201KDAT00 )

Headliner Removal/Installation

1. If necessary, remove the front grab handle bracket (A) and the rear grab handle bracket (B).
   NOTE:
   - The grab handle bracket was joined up the tab plates of the side curtain airbag. Prying the tab plates by force makes it possible to remove the bracket.
   - Take care not to damage the side curtain airbag.

   -1. | Remove the bolts (C, D, E).
   -2. | With a flat-tip screwdriver, carefully pry up a gap between the front tab plate (F) and the grab handle bracket to detach the joint (G).
   -3. | Repeat preceding step at the rear tab plate (H) portion to detach the plate from the bracket.
   -4. | Detach the clips (I).

Front
Rear