( TL19E00R11100000000YCAT10 )

Floor and Rear Body Construction

NOTE: Confirm that the sold as repair parts, refer to the appropriate Parts Catalog.
NOTE:

- The part marked with numbers are sold as repair parts.
- The part marked with letters are not sold separately and are shown only for reference.
- [ ]: Thickness unit: mm (in.)
- High-tension steel sheet: Tensioner strength 340 to 590 MPa.

No. | Part Name | Tensioner Strength (MPa) | Zinc-plating
--- | --- | --- | ---
(1) | Front Floor Comp.
| a: | Front Floor [0.65 (0.026)] | 270 | ○
b: | Front Floor Frame | Front [1.4 (0.055)] | 590 |
Rear [1.2 (0.047)] | 590 |
c: | Floor Tunnel Frame [0.8 (0.031)] | 590 | ○
-1 | Front Inside Sill [1.4 (0.055)] | 590 | ○
d: | Inside Sill Reinforcement [1.4 (0.055)] Driver's Side | 590 | ○
(2) | Rear Floor Panel [0.65 (0.026)] | 270 | ○
(3) | Rear Bulkhead Lower Cross-member Comp.
| a: | Bulkhead Lower Cross-member [1.2 (0.047)] | 270 |
b: | Rear Upper Frame C [1.4 (0.055)] | 590 | ○
(4) | Spare Tyre Pan [0.7 (0.028)] | 270 | ○
-1 | Rear Jack Stiffener [1.8 (0.071)] | 270 | ○
(5) | Rear Frame Comp.
| a: | Rear Frame A [1.8 (0.071)] | 590 | ○
b: | Rear Frame B [1.6 (0.063)] | 590 | ○
-1 | Rear Frame C [1.4 (0.055)] | 590 | ○
-2 | Rear Frame End Plate [2.3 (0.091)] | 440 | ○
-3 | Rear Upper Frame Comp.
c: | Rear Upper Frame B [1.0 (0.039)] | 590 | ○
d: | Rear Floor Side Panel [0.65 (0.026)] | 270 | ○
-4 | Rear Panel Gusset [1.0 (0.039)] | 270 | ○
(6) | Middle Floor Cross-member Comp.
| a: | Middle Floor Cross-member [1.2 (0.047)] | 590 | ○
b: | Middle Floor Cross-member Stiffener [0.8 (0.031)] | 590 | ○
c: | Rear Frame Joint [1.8 (0.071)] | 590 | ○
(7) | Rear Floor Cross-member [1.0 (0.039)] | 270 | ○
| a: | Rear Floor Patch [1.0 (0.039)] | 590 | ○
(8) | Rear Panel Comp.
-1 | Rear Bumper Face Stiffener [1.0 (0.039)] | 270 | ○
| a: | Rear Panel [0.6 (0.024)] | 270 | ○
b: | Rear Combination Stiffener [0.8 (0.031)] | 270 |
(9) | Rear Parcel Shelf [0.6 (0.024)] | 270 |
(10) | Trunk Lid | Skin Upper [0.7 (0.028)], Lower [0.6 (0.024)] | 270 | ○
Frame [0.6 (0.024)] | 270 | ○