( TL19E00J18573465521KBAT00 )

Windshield Side Trim Replacement

Retainer Replacement

1. Gradually scrape off the adhesive tape (A) under the retainers (B) while heating it with a heat gun to about 100−120 °C (212−248 °F).
   NOTE:
   - To prevent damage, do not heat the painted surface around the retainers too much.
   - To keep the exterior resin parts near the front pillar from being overheated by the heat gun, wrap them with aluminum foil.

1. Clean the body bonding surface with a sponge dampened in isopropyl alcohol. After cleaning, keep oil, grease, and water from getting on the surface.