( TL19E1AE3415033911FMAAT00 )

M/T Shift Fork Clearance Inspection

1. Measure the thickness of the shift fork fingers.
   - If the thickness is not within the standard, replace the shift fork.
   - If the thickness is within the standard, replace the synchro sleeve and synchro hub as a set.
   - If one arm of the shift fork shows more wear than others, the fork may be bent and needs to be replaced.

   Standard: | 7.4−7.6 mm (0.29−0.30 in.)