( TL19E00J34600000000CAAT00 )

Exterior Lights
The passenger's MICU controls the front passenger's side headlight, position lights, daytime running lights (KG model) and front and rear fog lights based upon the input signals from the driver's MICU.

| Input | Output
--- | --- | ---
Passenger's MICU |  | Position light Headlight (high beam, low beam passing) Front fog light
B-CAN | Position light signal Headlight (high beam, low beam passing) signal Front fog light signal Daytime running lights signal Rear fog light signal | Rear fog light