( TL19E1PE10410612223FEAT10 )

A/T Clutch Pressure Control Solenoid Valve A Test

1. Disconnect the connector from A/T clutch pressure control solenoid valve A.

1. Measure the resistance between A/T clutch pressure control solenoid valve A connector terminals No. 1 and No. 2.

   Standard: | 3−10 Ω

   - If the resistance is within the standard, go to Step 7 .
   - If the resistance is out of standard, replace A/T clutch pressure control solenoid valve A.

1. Connect a jumper wire from the negative battery terminal to A/T clutch pressure control solenoid valve A connector terminal No. 2, and connect another jumper wire from the positive battery terminal to A/T clutch pressure control solenoid valve A connector terminal No. 1.
   - If a clicking sound is heard, the valve is OK. The test is complete, reconnect the connector, then go to Step 20 .
   - If no clicking sound is heard, go to Step 8 .