( TL19E00R311000K5352YDAT04 )

Front Pillar Outer Panel Removal

NOTE: This section explains the procedures after removal of all accessories and related parts. For accessories' and related parts' removal procedure, refer to the appropriate Shop Manual.
Mass production body welding position and number (Outer panel and front pillar lower stiffener)
NOTE:

- Welding symbols
  : 2-Plate spot welding/ : 3-Plate spot welding/ : 4-Plate spot welding/ : MIG plug welding/ : MIG welding L= Welding length Unit: mm (in.)
- ( ): The number of welds

Construction

- Remove the wheelhouse upper member.
- Cut and pry off the outer panel at the front pillar and side sill portion.
  NOTE: Select the cutting positions in consideration of the front side outer panel repair part.
- Replace the front pillar outer separator.
- Check the front pillar lower stiffener position for damage. If necessary, replace it.
- Replace the front pillar inner separator.