( TL19E00G10110200000KBAT00 )

A/C Condenser Replacement

1. Recover the refrigerant with a recovery/recycling/charging station.

1. Remove the front grille cover.

1. Remove the clips (A) and the air intake duct cover (B).

1. Remove the bolt, then disconnect the receiver pipe (A) from the A/C condenser.

1. Loosen the bolts (A) from the A/C condenser.

1. Remove the bolts and the radiator upper mount blackest (A).

1. Remove the bolt, then disconnect the discharge hose (A) from the A/C condenser.

1. Remove the bolts, then remove the A/C condenser (A) by lifting it up. Be careful not to damage the radiator or condenser fins when removing the A/C condenser.

1. Install the A/C condenser in the reverse order of removal, and note these items:
   - If you're installing a new A/C condenser, add refrigerant oil (SP-10).
   - Replace the O-rings with new ones at each fitting, and apply a thin coat of refrigerant oil before installing them. Be sure to use the correct O-rings for HFC-134a (R-134a) to avoid leakage.
   - Immediately after using the oil, reinstall the cap on the container, and seal it to avoid moisture absorption.
   - Do not spill the refrigerant oil on the vehicle; it may damage the paint; if the refrigerant oil contacts the paint, wash it off immediately.
   - Be careful not to damage the radiator or the A/C condenser fins when installing the A/C condenser.
   - Charge the system.