( TL19E00J54460647101FEAT00 )

Power Window Driver's Motor Test

1. Check for continuity between the door multiplex control unit 37P connector No. 12 and No. 24 terminals and the driver's power window motor 6P connector No. 1 and No. 4 terminals respectively. There should be continuity.

   DOOR MULTIPLEX CONTROL UNIT 37P CONNECTOR | DRIVER'S POWER WINDOW MOTOR 6P CONNECTOR
   --- | ---
   No. 12 terminal | No. 4 terminal
   No. 24 terminal | No. 1 terminal

1. If the wire harness is OK, replace the driver's power window motor.