( TL19E00H46400016251KBAT00 )

Cable Reel Replacement

1. Install and torque a new steering wheel bolt (A), then reconnect the connectors.

1. Install the driver's airbag.

1. Do the battery terminal reconnection procedure.

1. Connect the HDS and clear any DTCs.

1. After installing the cable reel, confirm proper system operation:
   - Turn the ignition switch to ON (II); the SRS indicator should come on for about 6 seconds and then go off.
   - After the SRS indicator has turned off, turn the steering wheel fully left and right to confirm the SRS indicator does not come on.
   - Make sure the horn works.
   - Make sure the cruise control buttons work.
   - Make sure the steering wheel audio controls work.
   - Make sure the INFO/SEL buttons works.
   - Make sure there are no DTCs.