( TL19E00B20200000000MBAT00 )

Wheel Alignment

Special Tools Required
Wheel alignment gauge attachment, 64 x 40 mm
07MGK-0010100
The suspension can be adjusted for front and rear toe.
Pre-Alignment Checks
For proper inspection and adjustment of the wheel alignment, do these checks:

1. Release the parking brake to avoid an incorrect measurement.

1. Make sure the suspension is not modified.

1. Make sure the fuel tank is full, and that the spare tyre or the temporary repair kit, the jack, and the tools are in place on the vehicle.

1. Check the tyre size and tyre pressure according to tyre information.

1. Check the runout of the wheels and tyres.

1. Check the suspension ball joints.
   - Ball joint boot inspection
   - Knuckle ball joint inspection

1. Before doing alignment inspections, be sure to remove all extra weight from the vehicle, and no one should be inside the vehicle (driver or passengers).

1. Bounce the vehicle up and down several times to stabilize the suspension.

1. Check that the steering column is set at the center tilt and telescopic position.