( TL19E00G10123725311KBAT00 )

A/C Evaporator Core Replacement

1. When the evaporator temperature sensor (A) is reinstalled onto a new evaporator core, set the evaporator temperature sensor in the 8th fin from the other side of expansion valve.
   NOTE: If you are installing the sensor onto the old evaporator core, install the sensor onto the 9th fin, because the 8th fin may be deformed from the previous installation.

1. Install the core in the reverse order of removal, and note these items:
   - If you're installing a new evaporator core, add refrigerant oil (SP-10).
   - Replace the O-rings with new ones at each fitting, and apply a thin coat of refrigerant oil before installing them. Be sure to use the correct O-rings for HFC-134a (R-134a) to avoid leakage.
   - Immediately after using the oil, reinstall the cap on the container, and seal it to avoid moisture absorption.
   - Do not spill the refrigerant oil on the vehicle; it may damage the paint; if the refrigerant oil contacts the paint, wash it off immediately.
   - Make sure that there is no air leakage.
   - Charge the system.