( TL19E00J46643421011FEAT00 )

Door Lock Knob Switch Test

Front Passenger's Door

1. Remove the passenger's door panel.

1. Disconnect the 10P connector (A) from the actuator (B).

1. Check for continuity between the terminals.
   There should be continuity between the No. 8 [No. 7] and No. 10 [No. 5] terminals when the door lock knob switch in the UNLOCK position and no continuity when the switch is in the LOCK position.
   [ ]: RHD model

1. If the continuity is not specified, replace the door lock actuator.