( TL19E00J54460600000CAAT00 )

Anti-pinch Power Window Operation
The system is composed of the driver's MICU, passenger's MICU unit, door multiplex control unit (built into the power window master switch), front passenger's power window switch * , left and right rear power window switches * , and power window motors.

*: | With all power windows AUTO UP/AUTO DOWN function

The power window motor incorporates a pulser which generates pulses during the motor's operation and sends pulses to the driver's and passenger's power window control unit. As soon as the power window control unit detects a change in the pulse frequency from the pulser, the power window control unit makes the power window motor stop and reverse. This prevents pinching your hand or fingers during auto-up operation.
Key Cylinder Operation
With the key inserted in the driver's door key cylinder, turn the key a second time within 10 seconds and hold it to operate the windows and sunroof (clockwise to open, counterclockwise to close). The windows and sunroof stop moving when the key is released. The anti-pinch operation is not active when closing the windows and sunroof with the key cylinder.
Keyless Operation
By pressing and holding the UNLOCK button of the keyless transmitter a second time within 10 seconds, the windows and sunroof open. The windows and sunroof stop moving when the UNLOCK button is released. For KQ model, the windows do not close with the LOCK button.