( TL19E20A20326400000BAAT00 )

Fuel Pressure Relieving

Without the HDS

1. Remove the driver's dashboard lower cover.

1. Remove the PGM-FI main relay 2 (A) from the driver's under-dash fuse/relay box.

1. Start the engine, and let it idle until it stalls.
   NOTE: If any DTCs are stored, clear and ignore them.

1. Turn the ignition switch to LOCK (0).

1. Remove the fuel fill cap to relieve the pressure in the fuel tank.

1. Do the battery terminal disconnection procedure.