( TL19E20A14600017801MAAT00 )

Cylinder Head Inspection for Warpage

1. Remove the cylinder head.

1. Inspect the camshaft.

1. Check the cylinder head for warpage. Measure along the edges, and three ways across the center.
   - If warpage is less than 0.08 mm (0.003 in.) cylinder head resurfacing is not required.
   - If warpage is between 0.08 mm (0.003 in.) and 0.2 mm (0.008 in.), resurface the cylinder head.
   - The maximum resurface limit is 0.2 mm (0.008 in.) based on a height of 115 mm (4.53 in.).

   Cylinder Head Height
   Standard (New): | 114.95−115.05 mm (4.526−4.530 in.)