( TL19E00000000000000JBAT22 )

Maintenance Schedule for Severe Conditions - Australia and New Zealand

Follow the severe conditions maintenance schedule if the customer's vehicle is driven MAINLY under one or more of the following conditions:

- Driving less than 8 km (5 miles) per trip or, in freezing temperatures, driving less than 16 km (10 miles) per trip.
- Driving in extremely hot over 35 °C (95 °F) conditions.
- Extensive idling, or long periods of stop-and-go driving.
- Towing trailer, driving with a car-top carrier, or driving in mountainous conditions.
- Driving on muddy, dusty, or de-iced roads.

NOTE: If the vehicle is driven OCCASIONALLY under severe conditions, follow the normal conditions maintenance schedule.

Service at the indicated distance or time whichever comes first | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
miles x 1,000 | 12.5 | 25.0 | 37.5 | 50.0 | 62.5 | 75.0 | 87.5 | 100.0 | 112.5 | 125.0
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
Replace engine oil | Every 5,000 km (3,125 miles) or 6 months
Replace engine oil filter | Every 10,000 km (6,250 miles) or 1 year
Replace air cleaner element Use normal conditions except in dusty conditions. | Every 30,000 km (18,750 miles)
Inspect valve clearance | Every 40,000 km (25,000 miles)
Replace fuel filter Replace fuel filter every 40,000 km (25,000 miles) or 2 years, if the fuel the customer uses is suspected to be contaminated. |  |  |  | ● |  |  |  | ● |  |
Replace spark plugs | Every 100,000 km (62,500 miles)
Inspect drive belt Look for cracks and damage, then check the position of the drive belt auto-tensioner indicator. |  | ● |  | ● |  | ● |  | ● |  | ●
Inspect idle speed |  |  |  |  |  | ● |  |  |  |
Replace engine coolant Use genuine Honda All Season Antifreeze/Coolant Type 2. | At 200,000 km (120,000 miles) or 10 years, then every 100,000 km (60,000 miles) or 5 years
Replace Manual Transmission Fluid Use genuine Honda MTF. |  |  | ● |  |  | ● |  |  | ● |
Replace Automatic Transmission Fluid Use genuine Honda ATF-Z1. |  |  | ● |  | ● |  | ● |  | ● |

Check front and rear brakes

- Check the brake pad and disc thickness. Check for damage or cracks.
- Check the calipers for damage, leaks, and tightness.

Every 10,000 km (6,250 miles) or 6 months

Replace brake fluid

- Use only DOT 3 or DOT 4 brake fluid. We recommend genuine Honda Brake Fluid.
- Check the brake fluid level is between upper and lower marks on the reservoir.

Every 3 years

Check parking brake adjustment Check the parking brake operation. | ● | ● |  | ● |  | ● |  | ● |  | ●
Check lights alignment Check the position of the headlights. | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●
Test drive (noise, stability, dashboard operation)
Rotate tyres Check tyre inflation and condition at least once per month. | Every 10,000 km (6,250 miles)

Visually inspect the following items:
- Check for correct installation and position, check for cracks, deterioration, rust, and leaks.
- Check tightness of screws, nuts, and joints. If necessary, retighten.

Tie-rod ends, steering gearbox, and boots

- Check rack grease and steering linkage.
- Check the boot for damage and leaking grease.

Every 10,000 km (6,250 miles) or 6 months

Suspension components

- Check the bolts for tightness.
- Check all dust covers for deterioration and damage.

Driveshaft boots

- Check the boot and boot band for cracks.
- Check rack grease.

Brake hoses and lines (including VSA lines) Check the master cylinder and VSA modulator-control unit and leakage. | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●

All fluid levels and condition of fluids
Check levels and check for leaks. If necessary, add.

- Engine coolant
- MTF
- ATF
- Brake fluid
- Clutch fluid
- Windshield washer fluid

Exhaust system Check the exhaust pipe and muffler for damage, leaks, and tightness.

Fuel lines and connections

- Check fuel lines for loose connections, cracks, and deterioration.
- Retighten loose connections and replace any damaged parts.