( TL19E00J26273413801KDAT00 )

Interior Trim Removal/Installation - Pillar Areas

1. Remove these items:
   - Rear seat cushion
   - Rear seat side bolster
   - Rear door opening seal, as needed

1. Fold the seat-back forward.

1. Hit the upper clip in the rear pillar trim (A) with a rubber mallet. The clip is located under the point where the triangle mark (B) on the edge of the trim indicates. Hitting the clip slides the projections (C) on the pin (D) and pushes it into the grommet (E) and against the body (F).
   NOTE: The grommet must be replaced with a new one when the rear pillar trim is reinstalled.