( TL19E00H32500036861MBAT00 )

LKAS Camera Aiming

1. Make sure ‘‘CAM'' of MID goes out.
   NOTE: The static camera aiming status can be confirmed in the MID and LKAS indicator as follows. If ‘‘CAM'' is displayed on MID the aiming is not finished, then retry the static camera aiming procedure first.

The static camera aiming status

STATE | (1)MID | (2)LKAS INDICATOR (ORANGE)
Aiming is completed | OFF | OFF
Aiming is failure | ‘‘CAM'' ON | ON

1. The static camera aiming was completed. Go to the next step for the dynamic camera aiming procedure.