( TL19E00B20200014201KBAT20 )

Front Knuckle Ball Joint Replacement

1. Remove the ball joint (A) from the knuckle (B) by pushing the ball joint upward with the ball joint attachment and the air hammer (C).
   NOTE:
   - When removing the ball joint, use the air hammer according to the equipment manufacturer's instructions.
   - When removing the ball joint, adjust the clearance between the ball joint housing and the attachment to remove the ball joint easily.