( TL19E00J46127053771KBAT00 )

Front Seat Torsion Bar Replacement

Manual Height Adjustable Seat
NOTE:

- Put on gloves to protect your hands.
- Take care not to tear the seams or damage the seat covers.
- LHD model is shown; RHD model is symmetrical.

1. Remove the front seat.

1. Adjust the seat to its maximum height.

1. Release the hook strips from both sides and under of the seat cushion frame, then loosen the seat cushion cover.

1. Lever a hook shaped end of the front seat torsion bar (A) down using a long-handled clip remover.