( TL19E00B20200036401KBAT00 )

Front Knuckle/Hub/Wheel Bearing Replacement

Exploded View
Special Tools Required
Ball joint remover, 28 mm
07MAC-SL00201
Hub dis/assembly tool, 42 mm
07GAF-SD40100
Bearing driver attachment, 72 x 75 mm
07746-0010600
Driver handle, 15 x 135 L
07749-0010000
Bearing driver attachment, 78 x 90 mm
07GAD-SD40101
Support base, 73 x 78/82.6 mm
07965-SD90100
Knuckle/Hub Replacement

1. Raise the front of the vehicle, and support it with safety stands in the proper locations.

1. Remove the wheel nuts and the front wheel.