( TL19E00K722000R3505FAAT00 )

DTC Troubleshooting: 35-05

DTC 35-05:
EPS Control Unit Internal Circuit (Main/Sub) (Initial Diagnosis)

1. Turn the ignition switch to ON (II).

1. Clear the DTC with the HDS.

1. Turn the ignition switch to LOCK (0).

1. Start the engine.

1. Wait 10 seconds or more.

1. Check for DTCs with the HDS.

Is DTC 35-05 indicated?

YES | - | Replace the EPS control unit. ■
NO | - | Intermittent failure, the system is OK at this time.■