( TL19E1PE10411412281KBAT00 )

A/T Shift Cable Replacement

1. Apply molybdenum grease to the hole in the bushing (A) in the shift cable end (B). Attach the shift cable end to the selector control lever (C), then insert the control pin (D) into the selector control lever hole through the shift cable end, and secure the control pin with the spring clip (E). Do not bend the shift cable excessively.

1. Install the shift cable bracket (F) with the bolts (G).

1. Install the shift cable cover (H).

1. Install the shift cable on the shift lever, and adjust the shift cable.