( TL19E1PE10411310041LDAT00 )

A/T 1st, 2nd, and 3rd Clutch Reassembly

Special Tools Required
Clutch spring compressor set
07LAE-PX40000
Clutch spring compressor attachment
07LAE-PX40100
Clutch spring compressor attachment
07HAE-PL50100
Clutch spring compressor bolt set 10
07GAE-PG40200
Snap ring pliers
07LGC-0010100
NOTE:

- Hold the spring compressor attachment in a vise with soft jaws. Be careful not to damage the clutch drum.
- Insert the spring retainer can be adjusted (center of tolerance) to prevent damaging the spring retainer oil seal.

1. Soak the clutch discs thoroughly in ATF for at least 30 minutes.

1. Install a new O-ring (A) in the 1st, 2nd, and 3rd clutch pistons (B), and install a new O-ring (C) on each clutch drum (D).