( TL19E00B20200036401KBAT00 )

Front Knuckle/Hub/Wheel Bearing Replacement

1. Press a new wheel bearing (A) into the knuckle (B) using the old bearing (C), a steel plate (D), the bearing driver attachment, the support base, and a press.
   NOTE:
   - Install the wheel bearing with the wheel speed sensor magnetic encoder (E) (brown color), toward the inside of the knuckle.
   - Remove any oil, grease, dust, metal debris, and other foreign material from the encoder surface.
   - Keep any magnetic tools away from the encoder surface.
   - Be careful not to damage the encoder surface when you insert the wheel bearing.